( TL19E00E16226600000KCAT00 )

Driveshaft Installation

1. Connect the front stabilizer link (A) to the lower arm, and loosely install a new flange nut. Hold the stabilizer link joint pin (B) with a hex wrench (C), and tighten the new flange nut (D).

1. Place a floor jack under the lower arm, and raise the suspension to load it with the vehicle's weight.
   NOTE: Do not put the floor jack under the ball joint.

1. Tighten the damper pinch bolt and the damper fork mounting nut while holding the damper fork mounting bolt to the specified torque values.