( TL19E00J46166453632KBAT00 )

Rear Seat Cushion Cover Replacement

NOTE:

- Put on gloves to protect your hands.
- Take care not to tear the seams or damage the seat covers.

1. Remove the seat cushion.

1. From under the seat cushion, release all the upholstery rings (A), and fold back the seat cushion cover (B).

1. Pull back the edge of the seat cushion cover (A) all the way around, and release the upholstery rings (B), then remove the seat cushion cover.

1. Install the cover in the reverse order of removal, and note these items:
   - To prevent wrinkles when installing a seat cushion cover, make sure the material is stretched evenly over the pad before securing the upholstery rings.
   - Replace any upholstery rings (A) you removed with new ones. Install them with commercially available upholstery ring pliers (B).