( TL19E00H46400043771KBAT00 )

OPDS Unit Replacement

Installation

1. Place the OPDS unit (A) on the seat-back frame. Tighten the two nuts (B), and connect the connectors (C) to the OPDS unit. Reinstall the cover (D).

1. Install the seat-back cover.

1. Install the front seat assembly, then connect the side airbag harness 2P connector.

1. Do the battery terminal reconnection procedure.

1. Set the seat-back in the normal position, and make sure there is nothing on the front passenger's seat.

1. Initialize the OPDS unit.

1. Confirm proper SRS operation: Turn the ignition switch to ON (II); the SRS indicator should come on for about 6 seconds and then go off.