( TL19E30A20336359401KDAT00 )

Throttle Body Removal/Installation

Do not insert your fingers into the installed throttle body when you turn the ignition switch to ON (II) or while the ignition switch is ON (II). If you do, you will seriously injure your fingers if the throttle valve is activated.

1. Remove the intake air duct (A).

1. Disconnect the throttle body connector (B).

1. Disconnect and plug the water bypass hoses (C).

1. Remove the throttle body (D).

1. Install the parts in the reverse order of removal with a new gasket (E), then refill the radiator with engine coolant.
   NOTE:
   - If you replace or clean the throttle body, go to Step 6 .
   - If you did not replace or clean the throttle body, this procedure is complete.
   - When torquing the screw of the hose band (F), align the edge of the hose band (G) with the mark (H) painted on the hose band.

Do not insert your fingers into the installed throttle body when you turn the ignition switch to ON (II) or while the ignition switch is ON (II). If you do, you will seriously injure your fingers if the throttle valve is activated.

1. Remove the intake air duct (A).

1. Disconnect the throttle body connector (B).

1. Disconnect and plug the water bypass hoses (C).

1. Remove the throttle body (D).

1. Install the parts in the reverse order of removal with a new gasket (E), then refill the radiator with engine coolant.
   NOTE:
   - If you replace or clean the throttle body, go to Step 6 .
   - If you did not replace or clean the throttle body, this procedure is complete.
   - When torquing the screw of the hose band (F), align the edge of the hose band (G) with the mark (H) painted on the hose band.

1. Connect the HDS to the data link connector (DLC) (A) located under the driver's side of the dashboard.

1. Turn the ignition switch to ON (II).

1. Reset the ECM/PCM with the HDS.

1. Select the ETCS TEST in the INSPECTION MENU with the HDS.

1. Select TP POSITION CHECK and clear the throttle position (TP) learned value.

1. Turn the ignition switch to LOCK (0).

1. Turn the ignition switch to ON (II), and wait 2 seconds without pressing the accelerator pedal.

1. Do the ECM/PCM idle learn procedure.