( TL19E00B20200000000MBAT00 )

Wheel Alignment

Front Camber Inspection

1. Turn the front wheels to the straight ahead position.

1. Raise the front of the vehicle, and remove the wheel caps.
   NOTE: Push out the cap on the aluminum wheel from the inside after removing the wheel.

1. Install the wheel alignment gauge attachment (A) and camber/caster gauge on the wheel hub.

1. Read the camber angle on the gauge with the bubble at the center of the gauge.

   Front camber angle:
   | With 16 inch wheels: 0 ° 02 '±30 '
   | With 17 inch wheels: 0 ° 00 '±30 '
   | With 18 inch wheels: 0 ° 03 '±30 '
   (Maximum difference between the right and left side: 0 ° 30 ')

   - If the measurement is within specifications, measure the rear camber.
   - If the measurement is not within specifications, check for bent or damaged suspension components.