( TL19E00F00000057111KDAT00 )

Steering Gearbox Removal and Installation

1. Install the washers (A) and flange bolts to the steering gearbox, then loosely tighten the flange bolts.
   NOTE: Make sure that the washers is in position correctly.

1. Tighten the front/driver's side of the flange bolt (B) to the specified torque.

1. Tighten the front/passenger's side of the flange bolt (C) to the specified torque.

1. Tighten the rear side of the flange bolt (D) to the specified torque.