( TL19E1PE10410459801KAAT00 )

A/T Housing and Shaft Assembly Removal

1. Align the spring pin (A) on the selector control shaft (B) with the transmission housing groove (C) by turning the selector control shaft with the selector control lever on the torque converter side.
   NOTE: Do not squeeze the end of the selector control shaft tips together when turning the selector control shaft.

1. Install the housing puller over the mainshaft, then remove the transmission housing.

1. Remove the countershaft shaft reverse gear and the needle bearing.

1. Remove the lock bolt securing the shift fork, then remove the shift fork with the reverse selector together.

1. Remove the selector control lever from the selector control shaft.