( TL19E00J26273460309KDAT00 )

Interior Trim Removal/Installation - Trunk Lid

Trunk Lid Hinge Trim - For Some Models
NOTE:

- Put on gloves to protect your hands.
- Take care not to bend or scratch the panel.
- When removing components, use the trim tools or equivalent.

1. Remove the trunk side trim panel, as needed:
   - With temporary repair kit/with compact spare tyre
   - With normal spare tyre

1. Detach the clips (B, C), then remove the trunk lid hinge trim A by detaching the hooks (D).