( TL19E1PE10410744858KBAT00 )

A/T Paddle Shifter + (Upshift Switch) Replacement

1. Disconnect the paddle shifter + (upshift switch) connector. Remove the screw (A) securing the paddle shifter + (upshift switch) (B).

1. Using a TORX T30 bit, remove the TORX bolt (C), then remove the paddle shifter + (upshift switch).

1. Install the new paddle shifter + (upshift switch) on the steering wheel.

1. Connect the paddle shifter + (upshift switch) connector securely, and install the connector in the connector holder.

1. Tighten a new TORX bolt to the specified torque.

1. Connect the connectors. Install the steering wheel trim, and secure the steering wheel trim with the screws.

1. Install the steering wheel rear cover, and secure the rear cover with the screws.

1. Install the steering wheel.