( TL19E1PE10480154501MEAT00 )

A/T Servo Body Disassembly, Inspection, and Reassembly

1. Clean all parts thoroughly in solvent, and dry them with compressed air. Blow out all passages.

1. Inspect the valve body for scoring and damage.

1. Check shift valve D for free movement. If it fails to slide freely, refer to the valve body repair procedure.

1. When removing and installing the shift solenoid valves, refer to the shift solenoid valves removal and installation.

1. Coat all parts with ATF during assembly.

1. Replace the O-rings with new ones.

SPRING SPECIFICATIONS

Springs | Standard (New)-Unit: mm (in.)
--- | ---
Wire Diameter | O.D. | Free Length | No. of Coils
A | Shift valve D spring | 0.8 (0.031) | 5.6 (0.220) | 28.1 (1.106) | 15.9
B | 4th accumulator spring B | 2.3 (0.091) | 12.2 (0.480) | 31.5 (1.240) | 6.6
C | 4th accumulator spring A | 2.4 (0.094) | 18.6 (0.732) | 49.0 (1.929) | 7.1
D | 2nd accumulator spring B (For R20A3 engine model) | 2.0 (0.079) | 10.6 (0.417) | 34.0 (1.339) | 8.0
| 2nd accumulator spring B (For K24Z3 engine model) | 2.1 (0.083) | 10.8 (0.425) | 34.0 (1.339) | 8.2
E | 2nd accumulator spring A (For R20A3 engine model) | 2.2 (0.087) | 16.6 (0.654) | 48.2 (1.898) | 8.5
| 2nd accumulator spring A (For K24Z3 engine model) | 2.1 (0.083) | 16.6 (0.654) | 48.7 (1.917) | 8.4
F | 5th accumulator spring | 2.5 (0.098) | 14.6 (0.575) | 29.9 (1.177) | 4.9

1. Clean all parts thoroughly in solvent, and dry them with compressed air. Blow out all passages.

1. Inspect the valve body for scoring and damage.

1. Check shift valve D for free movement. If it fails to slide freely, refer to the valve body repair procedure.

1. When removing and installing the shift solenoid valves, refer to the shift solenoid valves removal and installation.

1. Coat all parts with ATF during assembly.

1. Replace the O-rings with new ones.

SPRING SPECIFICATIONS

Springs | Standard (New)-Unit: mm (in.)
--- | ---
Wire Diameter | O.D. | Free Length | No. of Coils
A | Shift valve D spring | 0.8 (0.031) | 5.6 (0.220) | 28.1 (1.106) | 15.9
B | 4th accumulator spring B | 2.3 (0.091) | 12.2 (0.480) | 31.5 (1.240) | 6.6
C | 4th accumulator spring A | 2.4 (0.094) | 18.6 (0.732) | 49.0 (1.929) | 7.1
D | 2nd accumulator spring B (For R20A3 engine model) | 2.0 (0.079) | 10.6 (0.417) | 34.0 (1.339) | 8.0
| 2nd accumulator spring B (For K24Z3 engine model) | 2.1 (0.083) | 10.8 (0.425) | 34.0 (1.339) | 8.2
E | 2nd accumulator spring A (For R20A3 engine model) | 2.2 (0.087) | 16.6 (0.654) | 48.2 (1.898) | 8.5
| 2nd accumulator spring A (For K24Z3 engine model) | 2.1 (0.083) | 16.6 (0.654) | 48.7 (1.917) | 8.4
F | 5th accumulator spring | 2.5 (0.098) | 14.6 (0.575) | 29.9 (1.177) | 4.9