( TL19E00J22100030053BBAT00 )

Gauge Control Module Self-diagnostic Function

Switch Input Check At the initial stage of the self-diagnostic function, the beeper sounds intermittently. The beeper sounds continuously when any of the following switch inputs are switched from OFF to ON: Cruise control main, set/decel, resume/accel, switches, SEL/RESET switch, parking brake switch, and VSA OFF switch previous, next switch, CMBS OFF switch, LKAS switch, Distance switch, Headlight washer switch. |