( TL19E00D52100000000HAAT03 )

VSA activation indicator does not go off, and no DTCs are stored

Diagnostic procedure

1. Symptom troubleshooting.
2. Update the VSA modulator-control unit if it does not have the latest software, or substitute a known-good VSA modulator-control unit, then retest. If it is OK, the VSA modulator-control unit was updated, troubleshooting is complete. If the VSA modulator-control unit was substituted, replace the original VSA modulator-control unit.