( TL19E1AE34150200000MAAT00 )

M/T Countershaft Assembly Clearance Inspection

NOTE: Before inspection, make sure the special bolt is tightened to the specified torque.

1. Measure the clearance between 1st gear (A) and the distance collar (B) with a feeler gauge (C).
   - If the clearance is more than the service limit, go to Step 2 .
   - If the clearance is within the service limit, go to Step 4 .

   Standard: | 0.06−0.16 mm (0.002−0.006 in.)
   Service Limit: | 0.25 mm (0.010 in.)