( TL19E1PE10411212211MAAT00 )

A/T Clutch Clearance Inspection

1. Release the clutch end-plate to lower the clutch end-plate, then put the clutch compressor attachment on the clutch end-plate (A).

1. Press the clutch compressor attachment down with 147 N (15 kgf, 33 lbf) (B) using a force gauge, and read the dial indicator (C). The dial indicator reads the clearance (D) between the clutch end-plate and the top disc (E). Take measurements in at least three places, and use the average as the actual clearance.

   Clearance between Clutch End-Plate and Top Disc
   Service Limit
   R20A3 Engine Model:
   1st Clutch: | 1.28−1.48 mm (0.050−0.058 in.)
   2nd Clutch: | 0.88−1.08 mm (0.035−0.043 in.)
   3rd Clutch: | 0.93−1.13 mm (0.037−0.044 in.)
   4th Clutch: | 0.93−1.13 mm (0.037−0.044 in.)
   5th Clutch: | 0.93−1.13 mm (0.037−0.044 in.)
   K24Z3 Engine Model:
   1st Clutch: | 1.38−1.58 mm (0.054−0.062 in.)
   2nd Clutch: | 1.14−1.34 mm (0.045−0.053 in.)
   3rd Clutch: | 1.23−1.43 mm (0.048−0.056 in.)
   4th Clutch: | 0.93−1.13 mm (0.037−0.044 in.)
   5th Clutch: | 0.93−1.13 mm (0.037−0.044 in.)