( TL19E00J00061517368KBAT00 )

Parking and Back-up Sensor Replacement

1. Remove the front bumper or the rear bumper.

1. Pull out the harness clamp (A) from the parking/back-up sensor (B), and disconnect the 6P connector (C) from the parking and back-up sensor.

1. Push the lock tab (A) with a screwdriver, and pinch the tab (B), then pull out the parking and back-up sensor from the retainer (C).

1. Install the parking and back-up sensor in the reverse order of removal.