( TL19E1PE10411239421MAAT00 )

A/T Mainshaft 5th Gear Axial Clearance Inspection

1. Remove the mainshaft transmission housing bearing.

1. Install the thrust needle bearing (A), 5th gear (B), the needle bearing (C), the thrust needle bearing (D), the 41 x 68 mm thrust washer (E), the 4th/5th clutch (F), the 4th gear collar (G), and the transmission housing bearing (H) on the mainshaft (I). Do not install the O-rings during inspection.

1. Install the idler gear (J) on the mainshaft with a press, then install the conical spring washer (K) and the locknut (L).

1. Tighten the locknut to 29 N·m (3.0 kgf·m, 22 lbf·ft).