( TL19E00J26220230101KDAT00 )

Glove Box Removal/Installation

SRS components are located in this area. Review the SRS component locations and the precautions and procedures before doing repairs or service.
NOTE:

- Take care not to scratch the dashboard and its related parts.
- When removing components, use the trim tools or equivalent.
- LHD model is shown; RHD model is symmetrical.

1. Open the glove box.

1. Open the front door, and remove the passenger's dashboard side lid (A).

   -1. | Gently pull the rear edge of the lid outward by hand to release the hooks (B).
   -2. | Detach the clips and the hooks (C) by pulling the lid outward.
   -3. | Release the hooks (D, E).
   -4. | If equipped, disconnect the passenger's airbag cutoff switch connector (F).

1. Remove the passenger's dashboard trim

1. Close the glove box.