( TL19E00R311000K5352YDAT06 )

Center Pillar Outer Panel Removal

NOTE: This section explains the procedures after removal of all accessories and related parts. For accessories' and related parts' removal procedure, refer to the appropriate Shop Manual.
Mass production body welding position and number (Outer panel, center pillar stiffener and side sill reinforcement)
NOTE:

- Welding symbols
  : 2-Plate spot welding/ : 3-Plate spot welding/ : 4-Plate spot welding/ : MIG plug welding/ : MIG welding L= Welding length Unit: mm (in.)
- ( ): The number of welds

Construction

- If there is any damage to the center pillar, cut the (A) position and pry off the outer panel, and replace it.
  NOTE: Select the cutting positions in consideration of the front side outer panel repair part.
- Check the side sill reinforcement and center pillar stiffener position for damage.
- If necessary, cut the (B) position of the outer panel, and replace the center pillar stiffener.
- When replacing the side sill reinforcement, remove the front pillar lower stiffener, and carefully cut the (C) position at the side sill rear portion of the outer panel.
- Replace the front pillar outer and inner separators, and the center pillar outer and inner separators.