( TL19E00K761000N1305FAAT00 )

DTC Troubleshooting: 1305

DTC 1305:
Gyro Error 2: ECU Temp XX °C
NOTE:

- Check the vehicle battery condition first.
- Before you troubleshoot, make sure to follow the general troubleshooting information.
- Make sure the vehicle is parked outside and away from buildings.
- Aftermarket electronic devices located near the navigation unit or GPS antenna can potentially interfere with the operation of the navigation system.
- Do this test only when the trunk temperature is between −20 °C (−4 °F) to 70 °C (158 °F).

1. Clear the hard error code.

1. Turn the ignition switch to LOCK (0), and then back to ON (II).

1. Check for the hard error code.

Is DTC 1305 indicated?

YES | - | Replace the navigation unit. ■
NO | - | Intermittent failure, the system is OK at this time.■