( TL19E00F00000057101KDAT00 )

Steering Column Removal and Installation

1. Loosen the upper steering joint bolt (A), and remove the lower steering joint bolt (B). Disconnect the steering joint (C) by moving the steering joint toward the column. Do not disconnect the steering joint from the column shaft (D).
   NOTE:
   - If the center guide (E) is in place and has not moved, leave it in place.
   - If the center guide has moved or been removed, discard it.