( TL19E1PE10410424251KCAT00 )

A/T End Cover Installation

1. For K24Z3 engine model: Connect the transmission range switch connector (A) securely, then install the harness clamps (B) on the clamp bracket (C). Install the transmission range switch cover (D).

1. Check the fluid passage of A/T clutch pressure control solenoid valve A for contamination. If necessary, clean the A/T clutch pressure control solenoid valve body.

1. Clean the mounting surface and fluid passage of the transmission housing.