( TL19E00K722000R1201FAAT00 )

DTC Troubleshooting: 12-01

DTC 12-01:
Low/High VBU Voltage (Regular Diagnosis)

1. Turn the ignition switch to ON (II).

1. Check the BATTERY in the DATA LIST with the HDS.

Is there battery voltage?

YES | - | Intermittent failure, the system is OK at this time. Check for poor connections or loose terminals at the EPS control unit.■
NO | - | Go to Step 3 .

1. Turn the ignition switch to LOCK (0).

1. Check the No. 2-1 (EPS) (70 A) fuse in the under-hood fuse/relay box.

Is the fuse blown?

YES | - | Go to Step 5 .
NO | - | Reinstall the checked fuse, then go to Step 13 .

1. Disconnect the EPS control unit connector A (2P).

1. Check for continuity between EPS control unit connector A (2P) terminal No. 2 and body ground.

Is there continuity?

YES | - | Repair short to body ground in the wire between the EPS control unit and the No. 2-1 (EPS) (70 A) fuse in the under-hood fuse/relay box.■
NO | - | Install a new No. 2-1 (EPS) (70 A) fuse in the under-hood fuse/relay box, then go to Step 7 .

1. Reconnect the EPS control unit connector A (2P).

1. Turn the ignition switch to ON (II).

1. Clear the DTC with the HDS.

1. Turn the ignition switch to LOCK (0).

1. Start the engine.

1. Check for DTCs with the HDS.

Is DTC 12-01 indicated?

YES | - | Replace the EPS control unit. ■
NO | - | Troubleshooting is complete. If any other DTCs are indicated, go to the indicated DTC's troubleshooting.■

1. Disconnect the EPS control unit connector A (2P).

1. Measure the voltage between EPS control unit connector A (2P) terminal No. 2 and body ground.

Is there battery voltage?

YES | - | Check for loose terminals in the EPS control unit connectors, and repair if necessary. If no poor connections are found, replace the EPS control unit. ■
NO | - | Repair open in the wire between the EPS control unit and No. 2-1 (EPS) (70 A) fuse in the under-hood fuse/relay box.■