( TL19E00K722000R1201FAAT00 )

DTC Troubleshooting: 12-01

1. Measure the voltage between EPS control unit connector A (2P) terminal No. 2 and body ground.

Is there battery voltage?

YES | - | Check for loose terminals in the EPS control unit connectors, and repair if necessary. If no poor connections are found, replace the EPS control unit. ■
NO | - | Repair open in the wire between the EPS control unit and No. 2-1 (EPS) (70 A) fuse in the under-hood fuse/relay box.■