( TL19E00K791000R8561FAAT00 )

DTC Troubleshooting: 85-61, 85-62

1. Measure the resistance between the No. 12 terminal of the OPDS unit harness 18P connector and body ground. There should be 0−1.0 Ω

Is the resistance as specified?

YES | - | Go to Step 9 .
NO | - | Open between the No. 12 terminal of the OPDS unit harness 18P connector and body ground (G701) or poor connection at G701. ■

1. Do the battery terminal disconnection procedure , then wait for 3 minutes.

1. Disconnect SRS unit connector B (39P) from the SRS unit.