( TL19E00B44100019102KDAT00 )

Rear Damper/Spring Removal and Installation

1. Loosely install the new damper lower mounting bolt (A) on the bottom of the damper. Connect the stabilizer link (B) to the brake hose bracket (C) to the knuckle, and loosely install the new self-locking nut (D).

1. Place a floor jack under the connecting point of the knuckle and lower arm A, and raise the suspension to load with the vehicle's weight.

1. Tighten the damper lower mounting bolt and the self-locking nut while holding the joint pin (E) with the hex wrench (F) to the specified torque values.

1. Tighten the damper mounting nuts on top of the damper to the specified torque value.