( TL19E00J26220219301KDAT00 )

Dashboard Driver's Lower Cover Removal/Installation

NOTE:

- Take care not to scratch the dashboard and its related parts.
- When removing components, use the trim tools or equivalent.
- LHD model is shown; RHD model is symmetrical.

1. Loosen the tilt/telescopic lock lever, and adjust the steering column upward. Leave the lock lever still be loosened.

1. Remove the driver's dashboard lower cover (A).

   -1. | Open the driver's pocket (B), and remove the screw (C).
   -2. | Pull out the bottom of the cover to detach the clips (D).
   -3. | Pull out along the edge of the cover to detach the clips (E, F).

1. Disconnect the connectors, if equipped:
   - The head light adjuster switch connector (G)
   - The headlight washer switch connector, the corner sensor connector, or the headlight adjuster switch/corner sensor switch connector (H)
   - The VSA/CMBS OFF switch connector (I)
   - Some RHD models: The ultrasonic sensor switch connector or the ultrasonic sensor switch/tilt sensor switch connector