( TL19E00J4616185367CKBAT00 )

Front Seat Up-down Motor Motor Replacement

1. While holding the gear (A) perpendicular to the axle of the rear brake (B) by hand, install the rear brake to the rear brake bracket (C).
   NOTE:
   - If any interferences between inside gears are felt, remove the rear brake, and repeat on Step 15 .
   - If the rear brake is fully seated on the rear brake bracket with no interference, go to Step 17 .