( TL19E00E16226600000LDAT00 )

Driveshaft Reassembly

1. Inspect the length (A) of the driveshafts to the figure as shown, then adjust the boots to halfway between full compression and full extension.

Model | Left/Right Driveshaft | Specified Length (A)
--- | --- | ---
R20A3 engine model | M/T | Left | 559−564 mm (22.01−22.20 in.)
Right | 547−552 mm (21.54−21.73 in.)
A/T | Left | 557−562 mm (21.93−22.13 in.)
Right | 545−550 m (21.46−21.65 in.)
K24Z3 engine model | M/T | Left | 559−564 mm (22.01−22.20 in.)
Right | 481−486 mm (18.94−19.13 in.)
A/T | Left | 554−559 mm (21.81−22.01 in.)
Right | 480−485 mm (18.90−19.09 in.)

Left driveshaft
Right driveshaft