( TL19E00R311000K5352YDAT08 )

Rear Side Outer Panel Removal

NOTE: This section explains the procedures after removal of all accessories and related parts. For accessories' and related parts' removal procedure, refer to the appropriate Shop Manual.
Mass production body welding position and number (Outer panel and rear gutter)
NOTE:

- Welding symbols
  : 2-Plate spot welding/ : 3-Plate spot welding/ : 4-Plate spot welding/ : MIG plug welding/ : MIG welding L= Welding length Unit: mm (in.)
- ( ): The number of welds

Construction

- Cut and pry off the rear side outer panel, and replace it.
  NOTE: Select the cutting positions in consideration of the rear side outer panel repair part.
- Check the rear gutter position for damage. If necessary, replace it.
- Replace the wheel arch outer separator.