( TL19E1PK77100090967FAAT00 )

DTC Troubleshooting: P0967 (23)

1. Check for continuity between A/T clutch pressure control solenoid valve B connector terminal No. 2 and body ground.

Is there continuity?

YES | - | Go to Step 18 .
NO | - | Repair open in the wire between A/T clutch pressure control solenoid valve B and body ground (G101); R20A3 engine model, K24Z3 engine model, or repair poor ground (G101), then go to Step 12 .

1. Reconnect all connectors.

1. Turn the ignition switch to ON (II).

1. Clear the DTC with the HDS.

1. Start the engine, and wait for at least 1 second.

1. Check for Temporary DTCs or DTCs with the HDS.

Is DTC P0967 indicated?

YES | - | Check for poor connections or loose terminals between A/T clutch pressure control solenoid valve B and the PCM, then go to Step 1 .
NO | - | Go to Step 17 .

1. Monitor the OBD STATUS for P0967 in the DTCs MENU with the HDS.

Does the HDS indicate PASSED?

YES | - | Troubleshooting is complete. If any other Temporary DTCs or DTCs were indicated in Step 16 , go to the indicated DTC's troubleshooting.■
NO | - | If the HDS indicates FAILED, check for poor connections or loose terminals between A/T clutch pressure control solenoid valve B and the PCM, then go to Step 1 . If the HDS indicates NOT COMPLETED, go to Step 15 .

1. Reconnect all connectors.

1. Update the PCM if it does not have the latest software; R20A3 engine model, K24Z3 engine model, or substitute a known-good PCM.

1. Start the engine, and wait for at least 1 second.

1. Check for Temporary DTCs or DTCs with the HDS.

Is DTC P0967 indicated?

YES | - | Check for poor connections or loose terminals between A/T clutch pressure control solenoid valve B and the PCM. If the PCM was updated, substitute a known-good PCM, then go to Step 20 . If the PCM was substituted, go to Step 1 .
NO | - | Go to Step 22 .

1. Monitor the OBD STATUS for P0967 in the DTCs MENU with the HDS.

Does the HDS indicate PASSED?

YES | - | If the PCM was updated, troubleshooting is complete. If the PCM was substituted, replace the original PCM; R20A3 engine model, K24Z3 engine model. If any other Temporary DTCs or DTCs were indicated in Step 21 , go to the indicated DTC's troubleshooting.■
NO | - | If the HDS indicates FAILED, check for poor connections or loose terminals between A/T clutch pressure control solenoid valve B and the PCM. If the PCM was updated, substitute a known-good PCM, then go to Step 20 . If the PCM was substituted, go to Step 1 . If the HDS indicates NOT COMPLETED, go to Step 20 .