( TL19E00K738000U1282FAAT00 )

DTC Troubleshooting: U1282

DTC U1282:
Headlight Leveling Control Unit Lost Communication with Driver's MICU

1. Clear the DTCs with the HDS.

1. Turn the ignition switch to LOCK (0) and then back to ON (II).

1. Wait for 6 seconds or more.

1. Check for DTCs with the HDS.

Is DTC U1282 indicated?

YES | - | Replace the headlight leveling control unit .■
NO | - | Intermittent failure, the system is OK at this time. Check for loose or poor connections between the driver's under-dash fuse/relay box and the headlight leveling control unit.■