( TL19E00J54400020371KBAT10 )

Front Door Glass and Regulator Replacement

1. Disconnect the power door lock actuator connector (A) and the power mirror connectors (B), and detach the power mirror connector and the harness clip (C). Remove the plug caps (D).

1. Pass the wire harnesses (E) through the slits (F) in the plastic cover (G), then remove the plastic cover.
   NOTE: Remove the glue from the door surface. If the plastic cover is damaged or torn, replace it.