( TL19E1PE10410612223FEAT20 )

A/T Clutch Pressure Control Solenoid Valve B Test

1. Disconnect the connector (A) from A/T clutch pressure control solenoid valve C.

1. Remove the harness clamps (D) from the clamp brackets.

1. Remove the mounting bolts and A/T clutch pressure control solenoid valves B and C with the clamp bracket (E).

1. Remove the ATF joint pipes (F), the O-rings (G), and the gasket (H) from the transmission housing.

1. Check the fluid passage of A/T clutch pressure control solenoid valves B and C for contamination.
   If necessary, clean the A/T clutch pressure control solenoid valve body.