( TL19E00K75200081060FAAT00 )

DTC Troubleshooting: 6

LKAS Camera DTC 6:
Temperature Monitoring Circuit Malfunction

1. Clear the DTCs with the HDS.

1. Turn the ignition switch to LOCK (0), then turn it to ON (II).

1. Watch the LKAS indicator.

Does the LKAS indicator come on?

YES | - | Go to Step 4 .
NO | - | Go to Step 5 .

1. Check for DTCs with the HDS.

Is DTC 6 indicated?

YES | - | Check for loose terminals in the LKAS camera 10P connector and LKAS control unit 26P connector. If all connections are OK, replace the LKAS camera and LKAS control unit as a set.
NO | - | Troubleshoot the indicated DTC(s).■

1. Check for DTCs with the HDS.

Is DTC 7 or 8 indicated?

YES | - | Do the troubleshoot for DTC 7 or 8.■
NO | - | Intermittent failure, the system is OK at this time.■