( TL19E00J34356544041FHAT00 )

Power Mirror Switch Test/Replacement

1. Remove the driver's door panel.

1. Remove the armrest and switch panel from the door panel.

1. Disconnect the 13P connector (A) from the power mirror switch (B), then remove the two screws and power mirror switch.

1. Check for continuity between the terminals in each switch position according to the table.

1. If the continuity is not as specified, remove the screws and replace the power mirror switch.

Power mirror switch
Retract switch