( TL19E1PE10436436021FAAT00 )

A/T Interlock System - Key Interlock System Circuit Troubleshooting

1. Check for continuity between shift lever 6P connector terminals No. 1 and No. 2. Do not push the shift lever button.

Is there continuity?

YES | - | Replace the park pin switch; LHD model, RHD model. ■
NO | - | Go to Step 11 .

1. Disconnect driver's under-dash fuse/relay box connector F (33P).

1. Turn the ignition switch to ON (II).