( TL19E00K769000Y10A2FAAT00 )

DTC Troubleshooting: B10A2

DTC B10A2:
Driver's MICU (EEPROM) Error

1. Clear the DTCs with the HDS.

1. Turn the ignition switch to LOCK (0) and then back to ON (II).

1. Wait for 6 seconds or more.

1. Check for DTCs with the HDS.

Is DTC B10A2 indicated?

YES | - | Faulty driver's MICU, replace the driver's under-dash fuse/relay box.■
NO | - | Intermittent failure, the system is OK at this time.■