( TL19E20A18223800000KAAT00 )

Engine Removal

1. Remove the vacuum hose (A), vacuum line mounting bolt (B), and the front engine mount stop (C), then remove the front engine mount bolt (D).

1. Check that the engine/transmission is completely free of vacuum hoses, fuel and coolant hoses, and electrical wiring.

1. Slowly raise the engine/transmission assembly about 150 mm (6 in.). Check once again that all hoses and electrical wiring are disconnected and free from the engine/transmission.

1. Raise the engine all the way, and remove it from the vehicle.