( TL19E00R311000K5352YDAT10 )

Spare Tyre Pan/Rear Frame Removal

NOTE: This section explains the procedures after removal of all accessories and related parts. For accessories' and related parts' removal procedure, refer to the appropriate Shop Manual.
Mass production body welding position and number (Spare tyre pan and rear floor side panel)
NOTE:

- Welding symbols
  : 2-Plate spot welding/ : 3-Plate spot welding/ : 4-Plate spot welding/ : MIG plug welding/ : MIG welding L= Welding length Unit: mm (in.)
- ( ): The number of welds

Mass production body welding position and number (Rear frame and rear floor cross-member)
NOTE:

- Welding symbols
  : 2-Plate spot welding/ : 3-Plate spot welding/ : 4-Plate spot welding/ : MIG plug welding/ : MIG welding L= Welding length Unit: mm (in.)
- ( ): The number of welds

Construction

- Remove the spare tyre pan and the rear floor side panel, and replace them.
- If there is any damage to the rear frame, replace the rear frame C, and repair the rear upper frame B if possible.

Construction

- Check the rear upper frame B, the rear frame B, and the rear floor cross-member position for damage. If necessary, replace them.
- When replacing the rear upper frame B and the rear frame B, carefully remove the rear bulkhead lower cross-member and the rear upper frame C. Drill the spot weld joints (X) for the rear frame stiffener and the rear upper frame A.