( TL19E00K764000Y1134FAAT00 )

DTC Troubleshooting: B1134

DTC B1134:
Right Rear Power Window Motor Pulse A Error

1. Clear the DTC with the HDS.

1. Turn the ignition switch to LOCK (0) and then back to ON (II).

1. Open and close the right rear power window by using the right rear power window switch manually.

1. Check for DTCs with the HDS.

Is DTC B1134 indicated?

YES | - | Go to Step 5 .
NO | - | Intermittent failure, the system is OK at this time. Check for loose or poor connections.■

1. Turn the ignition switch to LOCK (0).

1. Disconnect the right rear power window motor 6P connector.

1. Turn the ignition switch to ON (II).

1. Measure the voltage between the right rear power window motor 6P connector No. 6 terminal and body ground.

Is there about 4.2 V?

YES | - | Replace the right rear power window switch.■
NO | - | Go to Step 9 .

1. Disconnect the right rear power window switch 14P connector.