( TL19E1PE10410613041FHAT00 )

ATF Temperature Sensor Test/Replacement

1. Disconnect the shift solenoid wire harness connector (A), then remove the bolt (B) securing the shift solenoid wire harness (C) from the transmission housing.

1. Measure the ATF temperature sensor resistance between shift solenoid wire harness connector terminals No. 6 and No. 7.

   Standard: | 50 Ω−25 kΩ

1. If the resistance is out of standard, replace the ATF temperature sensor and the shift solenoid wire harness; go to Step 17 . The ATF temperature sensor is not available separately from the shift solenoid wire harness. If the resistance is within the standard, the ATF temperature sensor and the shift solenoid wire harness are OK; go to Step 16 .

1. Install a new O-ring (D) on a shift solenoid wire harness, then install the shift solenoid wire harness in the transmission housing. Secure the shift solenoid wire harness with the bolt, go to Step 19 .