( TL19E00J54400065501KBAT00 )

Windshield Replacement

1. Pack adhesive into the cartridge without air pockets to ensure continuous delivery. Put the cartridge in a caulking gun, and run a bead of adhesive (A) to the windshield (B) along the edge of the molding (C) and rubber dams (D) as shown. Apply the adhesive within 30 minutes after applying the glass primer. Make a slightly thicker bead at each corner.

1. Use suction cups to hold the windshield over the opening, align it with the alignment marks made in Step 17 , and set it down on the adhesive. Lightly push on the windshield until its edges are fully seated on the adhesive all the way around.
   NOTE: Do not open or close any of the doors for about an hour until the adhesive is dry.

1. Scrape or wipe the excess adhesive off with a putty knife or towel. To remove adhesive from a painted surface or the windshield, wipe with a soft shop towel dampened with isopropyl alcohol.

1. After the adhesive has dried, spray water over the windshield and check for leaks. Mark leaking areas, and let the windshield dry, then seal with sealant. Let the vehicle stand for at least 4 hours after windshield installation. If the vehicle has to be used within the first 4 hours, it must be driven slowly.

1. Reinstall all remaining removed parts.
   NOTE: Advise the customer not to do the following things for 2 to 3 days:
   - Slam the doors with all the windows rolled up.
   - Twist the body excessively (such as when going in and out of driveways at an angle or driving over rough, uneven roads).