( TL19E1AE34150439755MBAT00 )

M/T Clutch Housing Mainshaft Thrust Clearance Adjustment

1. Attach the catch adapter (A) and base adapter (B) to the mainshaft as follows:
   - Back out the catch adapter bolt (C), and loosen the two hex bolts (D).
   - Fit the holder over the mainshaft so its lip is towards the transmission.
   - Align the catch adapter lip around the groove at the inside of the mainshaft splines, then tighten the hex bolts.

1. Fully seat the mainshaft by tapping its end with a plastic hammer.

1. Thread the catch adapter bolt in until it just contacts the wide surface of the base adapter.