( TL19E20A14600000000KCAT00 )

Cylinder Head Installation

1. Install the harness clamps (A) and the positive crankcase ventilation (PCV) hose (B).

1. Install the intake manifold.

1. Install the drive belt.

1. Do the battery terminal reconnection procedure.

1. After installation, check that all tubes, hoses and connectors are installed correctly.

1. Inspect for fuel leaks. Turn the ignition switch to ON (II) (do not operate the starter) so the fuel pump runs for about 2 seconds and pressurizes the fuel line. Repeat this operation three times, then check for fuel leakage at any point in the fuel line.

1. Refill the radiator with engine coolant, and bleed air from the cooling system with the heater valve open.

1. Do the crankshaft position (CKP) pattern clear/CKP pattern learn procedure.

1. Inspect the idle speed.

1. Inspect the ignition timing.