( TL19E00J46161854027FEAT20 )

Power Seat Motor Test - Front Passenger's

1. Test the motor by applying battery power and ground to the terminals according to the table. When the motor stops running, disconnect battery power immediately.

1. If the motor does not run or fails to run smoothly, replace the motor.
   - Slide motor
   - Recline motor
   - Front up-down motor
   - Rear up-down motor

Slide motor
Recline motor
Front up-down motor
Rear up-down motor