( TL19E00J3213493111AKBAT00 )

Headlight Leveling Motor Replacement

1. For right side, move the radiator reservoir.

1. Disconnect the 3P connector (A) from the headlight leveling motor, then turn the leveling motor (B) 45 ° counterwise to remove it.

1. Remove the headlight high beam bulb and pull the headlight reflector slightly, then remove the headlight leveling motor.

1. Install the headlight leveling motor in the reverse order of removal.

1. After installing, do the headlight initial position learning.