( TL19E00J10300013143KDAT00 )

Audio Switch Panel Removal/Installation

Without Navigation System
NOTE:

- Put on gloves to protect your hands.
- Take care not to scratch the dashboard and related parts.
- Lay a workshop towel under the parts when working on them to protect the face panel from scratches or other damage.
- Do not work in a dusty or dirty place.
- Discharge static electricity from your body before and during the work.
- Do not touch the circuit board with your bare hands.
- Do not work with dirty hands.
- Be careful not no fold the flat plate cable.
- Do not touch the terminal connector of the flat plate cable with your bare hands. (If you have touched it, wipe it off thoroughly.)

1. Remove these items:
   - Driver's center trim
   - Passenger's dashboard trim
   - Passenger's center trim
   - Center console panel
   - Climate control unit
   - Dashboard center pocket
   - Dashboard center vent
   - Audio unit
   - Hazard switch

1. Remove the audio switch panel (A).

1. Install the audio switch panel in the reverse order of removal, and note these items:
   - Make sure all the connectors and the antenna lead are secure.
   - Enter the anti-theft codes for the audio system.

1. Give the new anti-theft codes to the customer.