( TL19E00E16226600000LDAT00 )

Driveshaft Reassembly

Exploded View
Special Tools Required
Boot band tool,
KD-3191
or equivalent, commercially available
Boot band pliers,
Kent-Moore J-35910
or equivalent, commercially available
Boot band pliers, commercially available
NOTE: Refer to the Exploded View, as needed, during this procedure.
Inboard Joint Side

1. Wrap the splines with vinyl tape (A) to prevent damage to the inboard boot.

1. Install the inboard boot onto the driveshaft, then remove the vinyl tape. Be careful not to damage the inboard boot.