( TL19E00J26273413801KDAT00 )

Interior Trim Removal/Installation - Pillar Areas

1. Remove the center pillar upper trim (A).

   -1. | Pull the bottom of the trim back by hand to detach the lower hooks (B).
   -2. | Pull the bottom of the trim back to release the upper pin (C) from the hole in the body and the slider (D) from pin (E) on the front seat belt shoulder anchor adjuster.
   -3. | Pull the trim down to release the upper hooks (F) from the holes in the body.