( TL19E1PE10410424251KAAT00 )

A/T End Cover Removal

Special Tools Required
Spline shaft holder set
07PAB-0010001

1. Remove the three bolts (D) securing the ATF cooler inlet line/ATF filter (E), the ATF filter bracket bolts (F), the ATF cooler line bolts (G), and remove the ATF cooler line/ATF filter and the ATF filter brackets (H).

1. Remove the bolts (I) securing the ATF cooler outlet line (J).

1. Remove the ATF dipstick guide tube (K).

1. Remove A/T clutch pressure control solenoid valve A, then remove the ATF joint pipes, the O-rings, the ATF pipe, and the gasket.

1. Remove A/T clutch pressure control solenoid valves B and C with the clamp bracket, then remove the ATF joint pipes, the O-rings, and the gasket.

1. Remove the transmission range switch cover (L).

1. Remove the transmission range switch harness clamps (M) from the clamp bracket (N), then remove the transmission range switch (O).

1. Remove the end cover (15 bolts) (P), then clamp bracket, the dowel pins, the O-rings, and the end cover gasket.